EZConfig-Scanning

GETTING STARTED | NEW FEATURES
| FAQ | HELP | TECHNICAL KNOWLEDGE BASE
Back
Would you like to configure :
DISCONNECTED DEVICE
CONNECTED DEVICE
SERIAL DATA WINDOW
EZConfig-Scanning provides a wide range of programming functions that can be performed on a Honeywell scanning device connected to a computer. EZConfig-Scanning allows you to change programmed parameters, create and print programming bar codes and update device firmware.
Create New Configuration
OPEN EXISTING CONFIGURATION
CREATE NEW CONFIGURATION
Search Device Number / Name
By Category
Browse any Configuration
By Category

Note: Click the device category
Refresh
Extended Ping

Note: No device found.
Model: Serial No: Firmware No: Connection: Show License/Plug-in Info Checking For Updates...
Model: Serial No: Firmware No: Connection: Show License/Plug-in Info Checking For Updates...
Model: Serial No: Firmware No: Connection: Show License/Plug-in Info Checking For Updates...
Model: Serial No: Firmware No: Connection: Show License/Plug-in Info Checking For Updates...
Note: Click on the device to connect / disconnect
Back
Device Details
Device/Model : Serial Number : Firmware Number :
Checking For Updates...
Update from File
File Name:
Update from Web
Note: To obtain the latest firmware updates for your device, please contact Honeywell Technical Support NA | EMEA | LA | APAC or Contact 1-800-867-5309

Update from File
File Name:
Update from Web
Model: Serial No: Firmware No: Connection: Checking For Updates...
Model: Serial No: Firmware No: Connection: Checking For Updates...
Model: Serial No: Firmware No: Connection: Checking For Updates...
Note: To obtain the latest firmware updates for your device, please contact Honeywell Technical Support NA | EMEA | LA | APAC or Contact 1-800-867-5309
CONFIGURE DEVICE
UPDATE FIRMWARE
SCAN DATA WINDOW
DEVICE DETAILS
Scanner Device
Serial No: Firmware No:
Auxiliary Scanners
Integrated Device
Configuration History
Settings

Symbologies

Data Formatting

Imaging

Note: Click on the undo arrow to undo the change to a parameter.
Bar Code Generation
Settings
Media Format
Bar Code Type
GENERATE BAR CODE
OPEN CONFIG
SAVE CONFIG
SAVE TO DEVICE
SAVE AS TXT FILE
RESET TO DEFAULT
AUXILLARY SCANNER - 1900h
Quick Help
Command:
CAPTURE
ACCEPT
Image Type
Select Device
Image Dimension

| Delete | Format Type | Interface Type | Symbology | Length | Command Sequence
--- | --- | --- | --- | --- | --- | ---

|  | Primary | Any Terminal | All Symbologies |  | Editor

Prefix/Suffix Data Table

| Delete | Symbology | Prefix | Suffix
--- | --- | --- | --- | ---

|  | All Symbologies | Editor | Editor

Prefix Value
Finish

Please select from Character Set option below.

Insert ASCII

Control Chars Printable Chars Extended ASCII

Insert Keypress

US Keyboard(104 Keys) European Keyboard(105 Keys)
Rule Help : Select Actions from below and subsequent sub-action to form the rule.
Select an Action
Select a Sub-Action
Cancel Rule
Add / Update
Control Chars Printable Chars Extended ASCII
Command Sequence
Finish
Command Center Create Programming Bar Code
Command Type :
Menu Command
Raw Command
Non Menu Command
1D Bar Code View Details: Bar Code Command
Horizontal Size
10%
Vertical Size
10%
2D Bar Code View Details: Bar Code Command
Bar Code Size
20% Symbologies
Show Request/Response Tags Expand Control Characters Hex HID Keyboard Single Data Display
1D Bar Code 2D Bar Code
Title :
Comments :
Title :
Comments :
Port Number
Baud Rate
Parity Bits
Data Bits
Stop Bits
Hand Shaking
Scanner Status Indicators
CTS Active
DSR DTR CTS RTS DTR Active
Menu Command
Raw Command
Non Menu Command
Show Request/Response Tags Expand Control Characters Hex
Terms & Conditions | Privacy Statement | Contact Information
| About Ver: 4.5.25 © 2017 Honeywell Inc. All rights reserved

- Primary
- Alternate 1
- Alternate 2
- Alternate 3

Primary
Any Terminal
All Symbologies
Save current settings to a file and load another settings file.
Discard changes and load another settings file.

Save device settings to a file and load File settings in offline mode.
Discard changes and load File settings in offline mode.

Please select the device for which the text file belongs to

Please select the device for which the text file belongs to

Save current settings to the device and load settings file.
Save current settings to a file and load another settings file.
Discard current settings and load settings file.

Data Format Menu Command Undo/Modify X
For modifying a format command, please go to Data Formatter page.
Undo Data Format will clear user modifications and revert to the original Data Format.
Original Settings
Modified Settings
Undo Prefix Format will clear user modifications and revert to the original Prefix Format.
Original Settings
Modified Settings
Undo Suffix Format will clear user modifications and revert to the original Suffix Format.
Original Settings
Modified Settings
Failed Commands X
Writing to device succeeded but following commands were not written.
Commands out of range:
Commands not present in the device:
Save current workgroup settings to the device.
Save all workgroups settings to the device.

Power cycle the device in 12 seconds or
press Cancel to exit Force boot operation
Available Firmware Details X
License/Plug-in Info X
About EZConfig X
© 2017 Honeywell Inc.
ASCII Conversion Chart X
EZConfig Version Update X
New Version of EZConfig is available. Click here for more details
EZConfig Version Information X
© 2017 Honeywell Inc.