;/*++
;
;COPYRIGHT (C) 2014-2015 Honeywell Corp.
;
;Module Name:
;
;    honeywell_scanner_hid.INF
;
;Abstract:
;    INF file for configuring Honeywell scanner POS HID barcode interface
;    with a NULL driver.
;
;--*/
[Version]
Signature = "$Windows NT$"
Class=HIDCLASS
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
Provider=%HONEYWELL%
DriverVer=08/15/2017,1.0.0.10
CatalogFile = honeywell_scanner_hid.cat

[Manufacturer]
%Mfg%=HidDeviceList,NTx86,NTamd64

; For Win2K
[HidDeviceList]
; DisplayName                   Section           DeviceId
; -----------                   -------           --------
; Hand Held Product (HHP) Device
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0107
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0127
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0167
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0187
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_01C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_01E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0207
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0227
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0267
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0287
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02A7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0307
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0327
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0347
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0407
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0427
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0447
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0467
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0487
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04A7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0527
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0547
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0567

; Honeywell HBOS(Voyager)/Xenon based device
; Xenon-based, TERMID 131, REMIFC0
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0907
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0913&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0901&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_090F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0927
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0933&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0921&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_092F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0987
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0993&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0981&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_098F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0947
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0953&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0941&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_094F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0967
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0973&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0961&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_096F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09C7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09D3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09C1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09CF&MI_01
; HBOS/Voyager based
; HBOS based, TERMID 131, REMIFC0, USB HIDPOS (LOB)
; EXCEPTION-EXCEPTION-EXCEPTION:
; Honeywell N8600 Series Area Image Engine. IMX53 based:
; a/ follow HBOS PID convention for CDC-ACM, TERMID 130
; b/ follow Xenon PID convention for HID POS, TERMID 131
; c/ follow Xenon PID convention for HID KBD, TERMID 124
; Xenon-based, TERMID 131, REMIFC0
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09E7
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09F3&MI_00
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (REM)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09F3&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09EF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09E1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A07&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A27&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AA7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AB3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AA1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AAF&MI_01
;

%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F47
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F53&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F53&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F4F&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F4F&MI_02
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F41&MI_01
;

%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC7&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC7&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FCF&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC1&MI_02
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F27
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F33&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F33&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F21&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F2F&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F2F&MI_02
;


%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A67&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A47&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B07&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B47&MI_00
;
;33xx Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B67&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B6F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B61&MI_01
;
;Voyager 1400g Series. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B87&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B8F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B81&MI_01
;
;Genesis 7580 Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BF3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BE7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BEF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BE1&MI_01
;
;1280i. Xenon based, follows correct PID index conv
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C2F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C21&MI_01
;
; EXCEPTION-EXCEPTION-EXCEPTION:
; 4850DR Document Imager. IMX53 based:
; a/ follow HBOS PID convention for CDC-ACM, TERMID 130
; b/ follow Xenon PID convention for HID POS, TERMID 131
; c/ follow Xenon PID convention for HID KBD, TERMID 124
; Xenon-based, TERMID 131, REMIFC0
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C47
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C53&MI_00
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (REM)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C53&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C41&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C27&MI_00
;
;Voyager 1450g. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CB3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CA7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CAF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CA1&MI_01
;
;Granit 1980i. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C67&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C6F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C61&MI_01
;
;14XX Charge & Communication Base. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CCF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CC1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0D93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0D87&MI_00
;
;Voyager 1602g. Xenon based, follows correct PID index conv
; NO REMIFC1
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DB3
;%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DA7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DAF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
;%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DA1&MI_01
;
;1602 Honeywell Access Point. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DCF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DC1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DE7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DF3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DE1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DEF&MI_01
;
; Granit 1981i CCB. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E07&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E0F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E01&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E27&MI_00
;
;Honeywell N3600 Series Area Image Engine. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E47&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E41&MI_01
;
;Solaris 7980 Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E87&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E8F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E81&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EA7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EB3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EA1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EAF&MI_01
;
; Honeywell N660X Series Area Image Engine. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0ED3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0ECF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EC1&MI_01

;Xenon 1850g. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F07&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F0F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F01&MI_01

; YOUJIE Scanners
;
;YJHF500. Xenon based, follows correct PID index conv
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C53
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C47&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C41&MI_01
;
;YJHF360. HBOS based
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C33
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C27&MI_00


; Legacy Intermec Device
;%INTERMEC_hid_device.Desc%=          RawDevInstall,       HID\VID_067E&PID_0809


; For XP and later
[HidDeviceList.NTx86]
; Hand Held Product (HHP) Device
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0107
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0127
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0167
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0187
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_01C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_01E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0207
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0227
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0267
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0287
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02A7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0307
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0327
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0347
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0407
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0427
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0447
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0467
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0487
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04A7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0527
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0547
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0567

; Honeywell HBOS(Voyager)/Xenon based device
; Xenon-based, TERMID 131, REMIFC0
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0907
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0913&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0901&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_090F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0927
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0933&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0921&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_092F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0987
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0993&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0981&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_098F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0947
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0953&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0941&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_094F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0967
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0973&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0961&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_096F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09C7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09D3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09C1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09CF&MI_01
; HBOS/Voyager based
; HBOS based, TERMID 131, REMIFC0, USB HIDPOS (LOB)
; EXCEPTION-EXCEPTION-EXCEPTION:
; Honeywell N8600 Series Area Image Engine. IMX53 based:
; a/ follow HBOS PID convention for CDC-ACM, TERMID 130
; b/ follow Xenon PID convention for HID POS, TERMID 131
; c/ follow Xenon PID convention for HID KBD, TERMID 124
; Xenon-based, TERMID 131, REMIFC0
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09E7
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09F3&MI_00
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (REM)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09F3&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09EF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09E1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A07&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A27&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AA7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AB3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AA1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AAF&MI_01
;

%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F47
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F53&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F53&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F4F&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F4F&MI_02
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F41&MI_01

;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC7&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC7&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FCF&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC1&MI_02
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F27
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F33&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F33&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F21&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F2F&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F2F&MI_02

%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A67&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A47&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B07&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B47&MI_00
;
;33xx Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B67&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B6F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B61&MI_01
;
;Voyager 1400g Series. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B87&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B8F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B81&MI_01
;
;Genesis 7580 Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BF3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BE7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BEF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BE1&MI_01
;
;1280i. Xenon based, follows correct PID index conv
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C2F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C21&MI_01
;
; EXCEPTION-EXCEPTION-EXCEPTION:
; 4850DR Document Imager. IMX53 based:
; a/ follow HBOS PID convention for CDC-ACM, TERMID 130
; b/ follow Xenon PID convention for HID POS, TERMID 131
; c/ follow Xenon PID convention for HID KBD, TERMID 124
; Xenon-based, TERMID 131, REMIFC0
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C47
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C53&MI_00
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (REM)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C53&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C41&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C27&MI_00
;
;Voyager 1450g. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CB3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CA7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CAF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CA1&MI_01
;
;Granit 1980i. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C67&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C6F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C61&MI_01
;
;14XX Charge & Communication Base. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CCF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CC1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0D93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0D87&MI_00
;
;Voyager 1602g. Xenon based, follows correct PID index conv
; NO REMIFC1
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DB3
;%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DA7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DAF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
;%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DA1&MI_01
;
;1602 Honeywell Access Point. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DCF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DC1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DE7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DF3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DE1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DEF&MI_01
;
; Granit 1981i CCB. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E07&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E0F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E01&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E27&MI_00
;
;Honeywell N3600 Series Area Image Engine. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E47&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E41&MI_01
;
;Solaris 7980 Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E87&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E8F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E81&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EA7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EB3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EA1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EAF&MI_01
;
; Honeywell N660X Series Area Image Engine. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0ED3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0ECF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EC1&MI_01

;Xenon 1850g. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F07&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F0F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F01&MI_01

; YOUJIE Scanners
;
;YJHF500. Xenon based, follows correct PID index conv
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C53
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C47&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C41&MI_01
;
;YJHF360. HBOS based
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C33
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C27&MI_00


; Legacy Intermec Device
;%INTERMEC_hid_device.Desc%=          RawDevInstall,       HID\VID_067E&PID_0809

; For XP and later x64
[HidDeviceList.NTamd64]
; Hand Held Product (HHP) Device
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0107
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0127
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0167
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0187
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_01C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_01E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0207
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0227
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0267
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0287
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02A7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_02E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0307
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0327
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0347
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0407
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0427
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0447
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0467
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0487
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04A7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04C7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_04E7
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0527
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0547
%HHP_hid_device.Desc%=          RawDevInstall,       HID\VID_0536&PID_0567

; Honeywell HBOS(Voyager)/Xenon based device
; Xenon-based, TERMID 131, REMIFC0
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0907
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0913&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0901&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_090F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0927
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0933&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0921&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_092F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0987
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0993&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0981&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_098F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0947
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0953&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0941&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_094F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0967
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0973&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0961&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_096F&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09C7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09D3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09C1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09CF&MI_01
; HBOS/Voyager based
; HBOS based, TERMID 131, REMIFC0, USB HIDPOS (LOB)
; EXCEPTION-EXCEPTION-EXCEPTION:
; Honeywell N8600 Series Area Image Engine. IMX53 based:
; a/ follow HBOS PID convention for CDC-ACM, TERMID 130
; b/ follow Xenon PID convention for HID POS, TERMID 131
; c/ follow Xenon PID convention for HID KBD, TERMID 124
; Xenon-based, TERMID 131, REMIFC0
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09E7
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09F3&MI_00
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (REM)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09F3&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09EF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_09E1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A07&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A27&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AA7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AB3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AA1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0AAF&MI_01
;

%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F47
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F53&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F53&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F4F&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F4F&MI_02
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F41&MI_01
;

%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC7&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC7&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FCF&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0FC1&MI_02
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F27
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F33&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F33&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F21&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F2F&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F2F&MI_02

%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A67&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0A47&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B07&MI_00
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B47&MI_00
;
;33xx Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B67&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B6F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B61&MI_01
;
;Voyager 1400g Series. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B87&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B8F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0B81&MI_01
;
;Genesis 7580 Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BF3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BE7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BEF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0BE1&MI_01
;
;1280i. Xenon based, follows correct PID index conv
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C2F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C21&MI_01
;
; EXCEPTION-EXCEPTION-EXCEPTION:
; 4850DR Document Imager. IMX53 based:
; a/ follow HBOS PID convention for CDC-ACM, TERMID 130
; b/ follow Xenon PID convention for HID POS, TERMID 131
; c/ follow Xenon PID convention for HID KBD, TERMID 124
; Xenon-based, TERMID 131, REMIFC0
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C47
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (LOB)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C53&MI_00
; Xenon-based, TERMID 131, REMIFC1, USB HIDPOS (REM)
%HON_usb_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C53&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C41&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C27&MI_00
;
;Voyager 1450g. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CB3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CA7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CAF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CA1&MI_01
;
;Granit 1980i. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C73
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C67&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C6F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0C61&MI_01
;
;14XX Charge & Communication Base. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CCF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0CC1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0D93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0D87&MI_00
;
;Voyager 1602g. Xenon based, follows correct PID index conv
; NO REMIFC1
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DB3
;%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DA7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DAF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
;%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DA1&MI_01
;
;1602 Honeywell Access Point. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DD3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DCF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DC1&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DE7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DF3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DE1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0DEF&MI_01
;
; Granit 1981i CCB. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E07&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E0F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E01&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E33
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E27&MI_00
;
;Honeywell N3600 Series Area Image Engine. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E53
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E47&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E41&MI_01
;
;Solaris 7980 Area-Imaging Scanner. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E93
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E87&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E8F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0E81&MI_01
;
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EA7
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EB3&MI_00
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EA1&MI_01
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EAF&MI_01
;
; Honeywell N660X Series Area Image Engine. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0ED3
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EC7&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0ECF&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0EC1&MI_01

;Xenon 1850g. Xenon based, follows correct PID index conv
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F13
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F07&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F0F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%HON_hid_device.Desc%=          RawDevInstall,       HID\VID_0C2E&PID_0F01&MI_01

; YOUJIE Scanners
;
;YJHF500. Xenon based, follows correct PID index conv
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C53
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C47&MI_00
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC0. Legacy USB HID barcode
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C4F&MI_01
; Xenon-based, TERMID 124 (PC Keyboard), REMIFC1. Legacy USB HID barcode
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C41&MI_01
;
;YJHF360. HBOS based
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C33
%YOU_hid_device.Desc%=          RawDevInstall,       HID\VID_23D0&PID_0C27&MI_00


; Legacy Intermec Device
;%INTERMEC_hid_device.Desc%=          RawDevInstall,       HID\VID_067E&PID_0809

[DestinationDirs]
DefaultDestDir = 12    ; DIRID_DRIVERS

[SourceDisksNames]
3426 = %Disk1%

[SourceDisksFiles]
hidusb.sys 		= 3426
hidclass.sys 		= 3426
hidparse.sys 		= 3426


[RawDevInstall.NT]
; Nothing to do since this is a class filter
[RawDevInstall.NT.Services]
AddService = ,%SPSVCINST_ASSOCSERVICE% ; null service install

;
; Do nothing for Raw Devices.
;

[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
HON_hid_device.Desc = "Honeywell Scanner POS HID Barcode Scanner"
HHP_hid_device.Desc = "HHP Scanner POS HID Barcode Scanner"
YOU_hid_device.Desc = "Youjie Scanner POS HID Barcode Scanner"
INTERMEC_hid_device.Desc = "Intermec Scanner POS HID Barcode Scanner"
Mfg             = "Honeywell International, Inc."
HONEYWELL       = "Honeywell International, Inc."
Disk1           = "windows cd"
