# Reference Charts

## ASCII Conversion Chart (Code Page 1252)

In keyboard applications, ASCII Control Characters can be represented in 3 different ways, as shown below. The CTRL+X function is OS and application dependent. The following table lists some commonly used Microsoft functionality. This table applies to U.S. style keyboards. Certain characters may differ depending on your Country Code/PC regional settings.

Non-printable ASCII control characters | Keyboard Control + ASCII (CTRL+X) Mode
|  |  | Control + X Mode Off (KBDCAS0) | Windows Mode Control + X Mode On (KBDCAS2)
DEC | HEX | Char | CTRL + X | CTRL + X function
0 | 00 | NUL | Reserved | CTRL+ @ |
1 | 01 | SOH | NP Enter | CTRL+ A | Select all
2 | 02 | STX | Caps Lock | CTRL+ B | Bold
3 | 03 | ETX | ALT Make | CTRL+ C | Copy
4 | 04 | EOT | ALT Break | CTRL+ D | Bookmark
5 | 05 | ENQ | CTRL Make | CTRL+ E | Center
6 | 06 | ACK | CTRL Break | CTRL+ F | Find
7 | 07 | BEL | Enter / Ret | CTRL+ G |
8 | 08 | BS | (Apple Make) | CTRL+ H | History
9 | 09 | HT | Tab | CTRL+ I | Italic
10 | 0A | LF | (Apple Break) | CTRL+ J | Justify
11 | 0B | VT | Tab | CTRL+ K | hyperlink
12 | 0C | FF | Delete | CTRL+ L | list, left align
13 | 0D | CR | Enter / Ret | CTRL+ M |
14 | 0E | SO | Insert | CTRL+ N | New
15 | 0F | SI | ESC | CTRL+ O | Open
16 | 10 | DLE | F11 | CTRL+ P | Print
17 | 11 | DC1 | Home | CTRL+ Q | Quit
18 | 12 | DC2 | PrtScn | CTRL+ R |
19 | 13 | DC3 | Backspace | CTRL+ S | Save
20 | 14 | DC4 | Back Tab | CTRL+ T |
21 | 15 | NAK | F12 | CTRL+ U |
22 | 16 | SYN | F1 | CTRL+ V | Paste
23 | 17 | ETB | F2 | CTRL+ W |
24 | 18 | CAN | F3 | CTRL+ X |
25 | 19 | EM | F4 | CTRL+ Y |
26 | 1A | SUB | F5 | CTRL+ Z |
27 | 1B | ESC | F6 | CTRL+ [ |
28 | 1C | FS | F7 | CTRL+ \ |
29 | 1D | GS | F8 | CTRL+ ] |
30 | 1E | RS | F9 | CTRL+ ^ |
31 | 1F | US | F10 | CTRL+ - |
127 | 7F | ⌂ | NP Enter |  |

##

## Lower ASCII Reference Table

Note: Windows Code page 1252 and lower ASCII use the same characters.

Printable Characters
DEC | HEX | Character | DEC | HEX | Character | DEC | HEX | Character
32 | 20 | <SPACE> | 64 | 40 | @ | 96 | 60 | `
33 | 21 | ! | 65 | 41 | A | 97 | 61 | a
34 | 22 | " | 66 | 42 | B | 98 | 62 | b
35 | 23 | # | 67 | 43 | C | 99 | 63 | c
36 | 24 | $ | 68 | 44 | D | 100 | 64 | d
37 | 25 | % | 69 | 45 | E | 101 | 65 | e
38 | 26 | & | 70 | 46 | F | 102 | 66 | f
39 | 27 | ' | 71 | 47 | G | 103 | 67 | g
40 | 28 | ( | 72 | 48 | H | 104 | 68 | h
41 | 29 | ) | 73 | 49 | I | 105 | 69 | i
42 | 2A | * | 74 | 4A | J | 106 | 6A | j
43 | 2B | + | 75 | 4B | K | 107 | 6B | k
44 | 2C | , | 76 | 4C | L | 108 | 6C | l
45 | 2D | - | 77 | 4D | M | 109 | 6D | m
46 | 2E | . | 78 | 4E | N | 110 | 6E | n
47 | 2F | / | 79 | 4F | O | 111 | 6F | o
48 | 30 | 0 | 80 | 50 | P | 112 | 70 | p
49 | 31 | 1 | 81 | 51 | Q | 113 | 71 | q
50 | 32 | 2 | 82 | 52 | R | 114 | 72 | r
51 | 33 | 3 | 83 | 53 | S | 115 | 73 | s
52 | 34 | 4 | 84 | 54 | T | 116 | 74 | t
53 | 35 | 5 | 85 | 55 | U | 117 | 75 | u
54 | 36 | 6 | 86 | 56 | V | 118 | 76 | v
55 | 37 | 7 | 87 | 57 | W | 119 | 77 | w
56 | 38 | 8 | 88 | 58 | X | 120 | 78 | x
57 | 39 | 9 | 89 | 59 | Y | 121 | 79 | y
58 | 3A | : | 90 | 5A | Z | 122 | 7A | z
59 | 3B | ; | 91 | 5B | [ | 123 | 7B | {
60 | 3C | < | 92 | 5C | \ | 124 | 7C | |
61 | 3D | = | 93 | 5D | ] | 125 | 7D | }
62 | 3E | > | 94 | 5E | ^ | 126 | 7E | ~
63 | 3F | ? | 95 | 5F | _ | 127 | 7F | ⌂

Extended ASCII Characters
DEC | HEX | CP 1252 | ASCII | Alternate Extended | PS2 Scan Code
128 | 80 | € | Ç | up arrow ↑ | 0x48
129 | 81 |  | ü | down arrow ↓ | 0x50
130 | 82 | ‚ | é | right arrow → | 0x4B
131 | 83 | ƒ | â | left arrow ← | 0x4D
132 | 84 | „ | ä | Insert | 0x52
133 | 85 | … | à | Delete | 0x53
134 | 86 | † | å | Home | 0x47
135 | 87 | ‡ | ç | End | 0x4F
136 | 88 | ˆ | ê | Page Up | 0x49
137 | 89 | ‰ | ë | Page Down | 0x51
138 | 8A | Š | è | Right ALT | 0x38
139 | 8B | ‹ | ï | Right CTRL | 0x1D
140 | 8C | Œ | î | Reserved | n/a
141 | 8D |  | ì | Reserved | n/a
142 | 8E | Ž | Ä | Numeric Keypad Enter | 0x1C
143 | 8F |  | Å | Numeric Keypad / | 0x35
144 | 90 |  | É | F1 | 0x3B
145 | 91 | ‘ | æ | F2 | 0x3C
146 | 92 | ’ | Æ | F3 | 0x3D
147 | 93 | “ | ô | F4 | 0x3E
148 | 94 | ” | ö | F5 | 0x3F
149 | 95 | • | ò | F6 | 0x40
150 | 96 | – | û | F7 | 0x41
151 | 97 | — | ù | F8 | 0x42
152 | 98 | ˜ | ÿ | F9 | 0x43
153 | 99 | ™ | Ö | F10 | 0x44
154 | 9A | š | Ü | F11 | 0x57
155 | 9B | › | ¢ | F12 | 0x58
156 | 9C | œ | £ | Numeric Keypad + | 0x4E
157 | 9D |  | ¥ | Numeric Keypad - | 0x4A
158 | 9E | ž | ₧ | Numeric Keypad * | 0x37
159 | 9F | Ÿ | ƒ | Caps Lock | 0x3A
160 | A0 |  | á | Num Lock | 0x45
161 | A1 | ¡ | í | Left Alt | 0x38
162 | A2 | ¢ | ó | Left Ctrl | 0x1D
163 | A3 | £ | ú | Left Shift | 0x2A
164 | A4 | ¤ | ñ | Right Shift | 0x36
165 | A5 | ¥ | Ñ | Print Screen | n/a
166 | A6 | ¦ | ª | Tab | 0x0F
167 | A7 | § | º | Shift Tab | 0x8F
168 | A8 | ¨ | ¿ | Enter | 0x1C
169 | A9 | © | ⌐ | Esc | 0x01
170 | AA | ª | ¬ | Alt Make | 0x36
171 | AB | « | ½ | Alt Break | 0xB6
172 | AC | ¬ | ¼ | Control Make | 0x1D
173 | AD |  | ¡ | Control Break | 0x9D
174 | AE | ® | « | Alt Sequence with 1 Character | 0x36
175 | AF | ¯ | » | Ctrl Sequence with 1 Character | 0x1D
176 | B0 | ° | ░ |  |
177 | B1 | ± | ▒ |  |
178 | B2 | ² | ▓ |  |
179 | B3 | ³ | │ |  |
180 | B4 | ´ | ┤ |  |
181 | B5 | µ | ╡ |  |
182 | B6 | ¶ | ╢ |  |
183 | B7 | · | ╖ |  |
184 | B8 | ¸ | ╕ |  |
185 | B9 | ¹ | ╣ |  |
186 | BA | º | ║ |  |
187 | BB | » | ╗ |  |
188 | BC | ¼ | ╝ |  |
189 | BD | ½ | ╜ |  |
190 | BE | ¾ | ╛ |  |
191 | BF | ¿ | ┐ |  |
192 | C0 | À | └ |  |
193 | C1 | Á | ┴ |  |
194 | C2 | Â | ┬ |  |
195 | C3 | Ã | ├ |  |
196 | C4 | Ä | ─ |  |
197 | C5 | Å | í |  |
198 | C6 | Æ | ╞ |  |
199 | C7 | Ç | ╟ |  |
200 | C8 | È | ╚ |  |
201 | C9 | É | ╔ |  |
202 | CA | Ê | ╩ |  |
203 | CB | Ë | ╦ |  |
204 | CC | Ì | ╠ |  |
205 | CD | Í | ═ |  |
206 | CE | Î | ╬ |  |
207 | CF | Ï | ╧ |  |
208 | D0 | Ð | ╨ |  |
209 | D1 | Ñ | ╤ |  |
210 | D2 | Ò | ╥ |  |
211 | D3 | Ó | ╙ |  |
212 | D4 | Ô | ╘ |  |
213 | D5 | Õ | ╒ |  |
214 | D6 | Ö | ╓ |  |
215 | D7 | × | ╫ |  |
216 | D8 | Ø | ╪ |  |
217 | D9 | Ù | ┘ |  |
218 | DA | Ú | ┌ |  |
219 | DB | Û | █ |  |
220 | DC | Ü | ▄ |  |
221 | DD | Ý | ▌ |  |
222 | DE | Þ | ▐ |  |
223 | DF | ß | ▀ |  |
224 | E0 | à | α |  |
225 | E1 | á | ß |  |
226 | E2 | â | Γ |  |
227 | E3 | ã | π |  |
228 | E4 | ä | Σ |  |
229 | E5 | å | σ |  |
230 | E6 | æ | µ |  |
231 | E7 | ç | τ |  |
232 | E8 | è | Φ |  |
233 | E9 | é | Θ |  |
234 | EA | ê | Ω |  |
235 | EB | ë | δ |  |
236 | EC | ì | ∞ |  |
237 | ED | í | φ |  |
238 | EE | î | ε |  |
239 | EF | ï | ∩ |  |
240 | F0 | ð | ≡ |  |
241 | F1 | ñ | ± |  |
242 | F2 | ò | ≥ |  |
243 | F3 | ó | ≤ |  |
244 | F4 | ô | ⌠ |  |
245 | F5 | õ | ⌡ |  |
246 | F6 | ö | ÷ |  |
247 | F7 | ÷ | ≈ |  |
248 | F8 | ø | ° |  |
249 | F9 | ù | ∙ |  |
250 | FA | ú | · |  |
251 | FB | û | √ |  |
252 | FC | ü | ⁿ |  |
253 | FD | ý | ² |  |
254 | FE | þ | ■ |  |
255 | FF | ÿ |  |  |

## Symbology Charts

Note: “m” represents the AIM modifier character. Refer to International Technical Specification, Symbology Identifiers, for AIM modifier character details.
Prefix / Suffix entries for specific symbologies override the universal (All Symbologies, 99) entry.

### Linear Symbologies

| AIM | Honeywell
Symbology | ID | Possible modifiers (m) | ID | Hex
All Symbologies |  |  |  | 99
Codabar | ]Fm | 0-1 | a | 61
Code 11 | ]H3 |  | h | 68
Code 128 | ]Cm | 0, 1, 2, 4 | j | 6A
Code 32 Pharmaceutical (PARAF) | ]X0 |  | < | 3C
Code 39 (supports Full ASCII mode) | ]Am | 0, 1, 3, 4, 5, 7 | b | 62
TCIF Linked Code 39 (TLC39) | ]L2 |  | T | 54
Code 93 and 93i | ]Gm | 0-9, A-Z, a-m | i | 69
EAN | ]Em | 0, 1, 3, 4 | d | 64
EAN-13 (including Bookland EAN) | ]E0 |  | d | 64
EAN-13 with Add-On | ]E3 |  | d | 64
EAN-13 with Extended Coupon Code | ]E3 |  | d | 64
EAN-8 | ]E4 |  | D | 44
EAN-8 with Add-On | ]E3 |  | D | 44
GS1 |  |  |  |
GS1 DataBar | ]em | 0 | y | 79
GS1 DataBar Limited | ]em |  | { | 7B
GS1 DataBar Expanded | ]em |  | } | 7D
GS1-128 | ]C1 |  | I | 49
2 of 5 |  |  |  |
China Post (Hong Kong 2 of 5) | ]X0 |  | Q | 51
Interleaved 2 of 5 | ]Im | 0, 1, 3 | e | 65
Matrix 2 of 5 | ]X0 |  | m | 6D
NEC 2 of 5 | ]X0 |  | Y | 59
Straight 2 of 5 IATA | ]Rm | 0, 1, 3 | f | 66
Straight 2 of 5 Industrial | ]S0 |  | f | 66
MSI | ]Mm | 0, 1 | g | 67
Telepen | ]Bm |  | t | 74
UPC |  | 0, 1, 2, 3, 8, 9, A, B, C |  |
UPC-A | ]E0 |  | c | 63
UPC-A with Add-On | ]E3 |  | c | 63
UPC-A with Extended Coupon Code | ]E3 |  | c | 63
UPC-E | ]E0 |  | E | 45
UPC-E with Add-On | ]E3 |  | E | 45
UPC-E1 | ]X0 |  | E | 45
Add Honeywell Code ID |  |  |  | 5C80
Add AIM Code ID |  |  |  | 5C81
Add Backslash |  |  |  | 5C5C
Batch mode quantity |  |  | 5 | 35

## 2D Symbologies

| AIM | Honeywell
Symbology | ID | Possible modifiers (m) | ID | Hex
All Symbologies |  |  |  | 99
Aztec Code | ]zm | 0-9, A-C | z | 7A
Chinese Sensible Code (Han Xin Code) | ]X0 |  | H | 48
Codablock A | ]O6 | 0, 1, 4, 5, 6 | V | 56
Codablock F | ]Om | 0, 1, 4, 5, 6 | q | 71
Code 49 | ]Tm | 0, 1, 2, 4 | l | 6C
Data Matrix | ]dm | 0-6 | w | 77
GS1 | ]em | 0-3 |  |
GS1 Composite | ]em | 0-3 | y | 79
GS1 DataBar Omnidirectional | ]em |  | y | 79
MaxiCode | ]Um | 0-3 | x | 78
PDF417 | ]Lm | 0-2 | r | 72
MicroPDF417 | ]Lm | 3-5 | R | 52
QR Code | ]Qm | 0-6 | s | 73
Micro QR Code | ]Qm |  | s | 73

## Postal Symbologies

| AIM | Honeywell
Symbology | ID | Possible modifiers (m) | ID | Hex
All Symbologies |  |  |  | 99
Australian Post | ]X0 |  | A | 41
British Post | ]X0 |  | B | 42
Canadian Post | ]X0 |  | C | 43
China Post | ]X0 |  | Q | 51
InfoMail | ]X0 |  | , | 2c
Intelligent Mail Bar Code | ]X0 |  | M | 4D
Japanese Post | ]X0 |  | J | 4A
KIX (Netherlands) Post | ]X0 |  | K | 4B
Korea Post | ]X0 |  | ? | 3F
Planet Code | ]X0 |  | L | 4C
Postal-4i | ]X0 |  | N | 4E
Postnet | ]X0 |  | P | 50

## ISO 2022/ISO 646 Character Replacements

Code pages define the mapping of character codes to characters. If the data received does not display with the proper characters, it may be because the bar code being scanned was created using a code page that is different from the one the host program is expecting. If this is the case, select the code page with which the bar codes were created. The data characters should then appear properly.

Code Page Selection Method/Country | Standard | Keyboard Country | Honeywell Code Page Option
United States (standard ASCII) | ISO/IEC 646-IRV | n/a | 1
Automatic National Character Replacement | ISO/IEC 2022 | n/a | 2 (default)
Binary Code page | n/a | n/a | 3
Default “Automatic National Character replacement” will select the following Honeywell Code Page options for Code128, Code 39 and Code 93.
United States | ISO/IEC 646-06 | 0 | 1
Canada | ISO /IEC 646-121 | 54 | 95
Canada | ISO /IEC 646-122 | 18 | 96
Japan | ISO/IEC 646-14 | 28 | 98
China | ISO/IEC 646-57 | 92 | 99
Great Britain (UK) | ISO /IEC 646-04 | 7 | 87
France | ISO /IEC 646-69 | 3 | 83
Germany | ISO/IEC646-21 | 4 | 84
Switzerland | ISO /IEC 646-CH | 6 | 86
Sweden / Finland (extended Annex C) | ISO/IEC 646-11 | 2 | 82
Ireland | ISO /IEC 646-207 | 73 | 97
Danmark | ISO/IEC 646-08 | 8 | 88
Norway | ISO/IEC 646-60 | 9 | 94
Italy | ISO/IEC 646-15 | 5 | 85
Portugal | ISO/IEC 646-16 | 13 | 92
Spain | ISO/IEC 646-17 | 10 | 90
Spain | ISO/IEC 646-85 | 51 | 91

Dec | 35 | 36 | 64 | 91 | 92 | 93 | 94 | 96 | 123 | 124 | 125 | 126
Hex | 23 | 24 | 40 | 5B | 5C | 5D | 5E | 60 | 7B | 7C | 7D | 7E
US | 0 | 1 | # | $ | @ | [ | \ | ] | ^ | ` | { | | | } | ~
CA | 54 | 95 | # | $ | à | â | ç | ê | î | ô | é | ù | è | û
CA | 18 | 96 | # | $ | à | â | ç | ê | É | ô | é | ù | è | û
JP | 28 | 98 | # | $ | @ | [ | ¥ | ] | ^ | ` | { | | | } | ‾
CN | 92 | 99 | # | ¥ | @ | [ | \ | ] | ^ | ` | { | | | } | ‾
GB | 7 | 87 | £ | $ | @ | [ | \ | ] | ^ | ` | { | | | } | ˜
FR | 3 | 83 | £ | $ | à | ° | ç | § | ^ | µ | é | ù | è | ¨
DE | 4 | 84 | # | $ | § | Ä | Ö | Ü | ^ | ` | ä | ö | ü | ß
CH | 6 | 86 | ù | $ | à | é | ç | ê | î | ô | ä | ö | ü | û
SE/FI | 2 | 82 | # | ¤ | É | Ä | Ö | Å | Ü | é | ä | ö | å | ü
DK | 8 | 88 | # | $ | @ | Æ | Ø | Å | ^ | ` | æ | ø | å | ˜
NO | 9 | 94 | # | $ | @ | Æ | Ø | Å | ^ | ` | æ | ø | å | ¨
IE | 73 | 97 | £ | $ | Ó | É | Í | Ú | Á | ó | é | í | ú | á
IT | 5 | 85 | £ | $ | § | ° | ç | é | ^ | ù | à | ò | è | ì
PT | 13 | 92 | # | $ | § | Ã | Ç | Õ | ^ | ` | ã | ç | õ | °
ES | 10 | 90 | # | $ | § | ¡ | Ñ | ¿ | ^ | ` | ° | ñ | ç | ˜
ES | 51 | 91 | # | $ | · | ¡ | Ñ | Ç | ¿ | ` | ´ | ñ | ç | ¨

COUNTRY

Country Keyboard

Honeywell CodePage

## ISO / IEC 646 National Character Replacements

## Unicode Key Maps

104 Key U.S. Style Keyboard

105 Key European Style Keyboard