zMIME-Version: 1.0
Content-Type: Multipart/Related;boundary=MIME_boundary;
    type="application/xop+xml";
    start="<RMLMessage.xml@honeywell.com>";
    start-info="text/xml"
Content-Description: An XML document with firmware and intsallation binary files

--MIME_boundary
Content-Type: application/xop+xml; 
    charset=UTF-8; 
    type="text/xml"
Content-Transfer-Encoding: 8bit
Content-ID: <RMLMessage.xml@honeywell.com>

<?xml version="1.0" encoding="ascii" standalone="no" ?>
<RML version="3.0" xmlns="http://www.honeywell.com/ReM/Information/Language/Protocols/RML" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://www.honeywell.com/ReM/Information/Language/Protocols/RMLExampleRMLSchema.xsd">
<!--Version - 4.0.1.6 -->
  <Boundary>
    <Name>Namespace
      <Value>ReM3.0.1</Value>
    </Name>
    <Name>DateTime
      <Value>2011-10-20T09:30:10-05:00</Value>
    </Name>
  </Boundary>

  <Origin>
    <Name>ReM Stack Layer
      <Value>Server</Value>
    </Name>
  </Origin>

  <Destination>
    <Name>Model
      <Value>HPA</Value>
    </Name>
    <Name>ReM Stack Layer
      <Value>HPA</Value>
    </Name>
    <Name>Serial Number
      <Value>{07CAA55E-F6CA-4D4C-BAA1-197DA4564B9B}</Value>
    </Name>
  </Destination>

  <Commands>
    <Name>Set Property
      <Nouns>
        <Name>Transport Configuration File
          <Value>
			<xop:Include xmlns:xop='http://www.w3.org/2004/08/xop/include' href='cid:http://honeywell.com/TransportConfigurationFile.rml'/>
           </Value>
        </Name>
		<Name>Access Connection
          <Value>
			<xop:Include xmlns:xop='http://www.w3.org/2004/08/xop/include' href='cid:http://honeywell.com/AccessConnection.rml'/>
           </Value>
        </Name>
        <Name>Logging Level
          <Value>1</Value>
        </Name>
        <Name>Max File Size
          <Value>1MB</Value>
        </Name>
        <Name>Max History Size
          <Value>5</Value>
        </Name>
        <Name>HPA Uses USB Barcode
          <Value>1</Value>
        </Name>
        <Name>HPA Uses USB IBM
          <Value>1</Value>
        </Name>
        <Name>HPA Uses RS232
          <Value>1</Value>
        </Name>
        <Name>HPA Uses USB Serial
          <Value>1</Value>
        </Name>
        <Name>HPA Uses USB Keyboard
          <Value>1</Value>
        </Name>
		<Name>HPA Uses Virtual COM
          <Value>0</Value>
        </Name>
        <Name>HPA Info Level
          <Value>Normal</Value>
        </Name>
        <Name>Maximum Discovery
          <Value>0</Value>
        </Name>
        <Name>HPA LOB Interface
          <Value>1</Value>
        </Name>
        <Name>HPA ReM Interface
          <Value>1</Value>
        </Name>
        <Name>HPA Legacy Interface
          <Value>1</Value>
        </Name>
        <Name>Timeout for Discovery
          <Value>70000</Value>
        </Name>
        <Name>HPA RS232 Baud Rates
          <Value>115200;57600;38400;19200;9600</Value>
        </Name>
        <Name>HPA DPS
          <Value>8N1;7N1;7N2;7E1;7E2;8E1;7O1;7O2;8O1</Value>
        </Name>
        <Name>Barcode Compatibility Level
          <Value>1</Value>
        </Name>		 
		<Name>Discovery Interval 
		 <Value>20</Value>
		</Name>
		<Name>Hub Refresh Interval
		 <Value>1</Value>
		</Name>
		<Name>SDK Logging Level
			<Value>0</Value>
		</Name>
		<Name>Hub Model Names
          <Value>CCB;AP;NGB;CCB00;CCB01;CCB02;2700;Stratos 2700;IT2020;2020;CCB00bf;CCB04;CCB05;AP01;CCB03;CCB06;CCB07;CCB08,CCB09;CCB10;AP02;AP03;AP04;AP05;AP06;AP07;AP08;AP09;AP10;AP100;XenonBFBase</Value>
        </Name>
		<Name>Flash One At A Time
			<Value>1</Value>
		</Name>
		<Name>MaskInternalDevices
			<Value>1</Value>
        </Name>
        <Name>MaskVirtualDevices
          <Value>1</Value>
        </Name>	
		<Name>Legacy Refresh
          <Value>1</Value>
        </Name>
		<Name>Bioptic Hub Models
          <Value>NGB;2700;Stratos 2700</Value>
        </Name>
		<Name>Connection Heartbeat
          <Value>0</Value>
        </Name>
        <Name>Config ID
          <Value>0</Value>
        </Name>
        <Name>Default Interface
          <Value>REM</Value>
        </Name>
		<Name>Allow LOB Connection
          <Value>1</Value>
        </Name>
		 <Name>AutoDiscovery
          <Value>0</Value>
        </Name>
		 <Name>Device Connection Timeout
          <Value>0</Value>
        </Name>
		 <Name>Turn On REMIFC
          <Value>0</Value>
        </Name>
        <Name>Packed XOP
          <Value>0</Value>
        </Name>
		<Name>RMLNamespace
		 <Value>ReM3.0.1</Value>
		</Name>
		<Name>Legacy Refresh Interval
          <Value>180</Value>
        </Name>
		 <Name>Send PropertyRequested On Connect
          <Value>0</Value>
        </Name>
		<Name>Discovery Serial Mask
          <Value>CTS;DSR;RING;RLSD</Value>
        </Name>
        <Name>Connection Serial Mask
          <Value>CTS;DSR;RING;RLSD</Value>
        </Name>
		<Name>Hubs Managing Sub Devices
		  <Value>CCB;AP;NGB;CCB00;CCB01;CCB02;2700;Stratos 2700;IT2020;2020;CCB00bf;CCB04;CCB05;AP01;CCB03;CCB06;CCB07;CCB08,CCB09;CCB10;AP02;AP03;AP04;AP05;AP06;AP07;AP08;AP09;AP10;AP100</Value>
        </Name>
		 <Name>Discard Original
          <Value>1</Value>
        </Name>
		<Name>Flash DLL Logging Level
          <Value>0</Value>
        </Name>
		<Name>Extended PING
          <Value>0</Value>
        </Name>
		<Name>Query License
          <Value>1</Value>
        </Name>
		<Name>Query Plugin
          <Value>1</Value>
        </Name>
        <Name>PING Settings Groups
          <Nouns>

            <Name>PING Settings Group
    
              <Nouns>
                <Name>PING Setting
        
                  <Value>115200;8N1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>9600;8N1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>115200;7E1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>9600;7E1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>38400;8N1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>57600;8N1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>19200;8N1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>38400;7E1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>57600;7E1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>19200;7E1;NORMAL</Value>
                </Name>
              </Nouns>
            </Name>

            <Name>PING Settings Group
    
              <Nouns>
                <Name>PING Setting
        
                  <Value>9600;7E2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>9600;7O1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>115200;7E2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>115200;7O1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>115200;7N1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>115200;7N2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>115200;8E1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>115200;7O2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>115200;8O1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>9600;7N1;NORMAL</Value>
                </Name>
              </Nouns>
            </Name>

            <Name>PING Settings Group
    
              <Nouns>
                <Name>PING Setting
        
                  <Value>9600;7N2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>9600;8E1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>9600;7O2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>9600;8O1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>38400;7E2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>38400;7O1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>38400;7N1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>38400;7N2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>38400;8E1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>38400;7O2;NORMAL</Value>
                </Name>
              </Nouns>
            </Name>
			<Name>PING Settings Group
    
              <Nouns>
			<Name>PING Setting
        
                  <Value>38400;8O1;NORMAL</Value>
                </Name>
			  <Name>PING Setting
        
                  <Value>57600;7E2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>57600;7O1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>57600;7N1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>57600;7N2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>57600;8E1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>57600;7O2;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>57600;8O1;NORMAL</Value>
                </Name>
                <Name>PING Setting
        
                  <Value>19200;7E2;NORMAL</Value>
                </Name>
				<Name>PING Setting
        
                  <Value>19200;7O1;NORMAL</Value>
                </Name>
                
              </Nouns>
            </Name>
			<Name>PING Settings Group
    
              <Nouns>
			
				<Name>PING Setting
						
                  <Value>19200;7N1;NORMAL</Value>
                </Name>
				<Name>PING Setting
						
                  <Value>19200;7N2;NORMAL</Value>
                </Name>
				<Name>PING Setting
						
                  <Value>19200;8E1;NORMAL</Value>
                </Name>
				<Name>PING Setting
						
                  <Value>19200;7O2;NORMAL</Value>
                </Name>
				<Name>PING Setting
						
                  <Value>19200;8O1;NORMAL</Value>
                </Name>
				
				 </Nouns>
            </Name>
          </Nouns>
        </Name>
		<Name>REMENA3 Notifications
			<Nouns>
			</Nouns>
    </Name>
		<Name>Notification Transforms
        <Nouns>
					<Name>Transform
						<Nouns>
						</Nouns>
					</Name>
				</Nouns>
    </Name>
	</Nouns>
  </Name>
    <Subject>
      <Name>Model
        <Value>HPA</Value>
      </Name>
      <Name>ReM Stack Layer
        <Value>HPA</Value>
      </Name>
      <Name>Serial Number
        <Value>{07CAA55E-F6CA-4D4C-BAA1-197DA4564B9B}</Value>
      </Name>
    </Subject>
  </Commands>

</RML>

--MIME_boundary
Content-Type: application/octet-stream
Content-Transfer-Encoding: binary
Content-ID: <http://honeywell.com/TransportConfigurationFile.rml>

<configuration><Config><type>server</type><port>9998</port><ip>0.0.0.0</ip><stayconnected>3000</stayconnected><blockenvelop>RMLDATA</blockenvelop><TransportFrequency>5</TransportFrequency><TransportStartTime>2011-10-20</TransportStartTime><TransportIsRealTime>1</TransportIsRealTime><NounCompatibilityLevel>1</NounCompatibilityLevel><NotificationCompatibilityLevel>2</NotificationCompatibilityLevel><CommandCompatibilityLevel>3</CommandCompatibilityLevel><protocol>TCPIP</protocol><JSTTLConnectionTimeout>120</JSTTLConnectionTimeout></Config><Logging><FileName>Log.log</FileName><LogLevel>1</LogLevel><Size Storage="MB">1</Size><NoOfFile>5</NoOfFile></Logging></configuration> 

--MIME_boundary
Content-Type: application/octet-stream
Content-Transfer-Encoding: binary
Content-ID: <http://honeywell.com/AccessConnection.rml>

<configuration>
	<Config>
		<type>client</type>
		<port>9992</port>
		<ip>127.0.0.1</ip>
		<stayconnected>3000</stayconnected>
		<protocol>HTTP</protocol>
		<blockenvelop>RMLDATA</blockenvelop>
		<ConnectionTimeout>1800</ConnectionTimeout>
		<pollingInterval>300</pollingInterval>
		<TryToConnect>TRUE</TryToConnect>
	</Config>
	<Logging>
		<FileName>D:\LOG\Clientlog.log</FileName>
		<LogLevel>1</LogLevel>
		<Size Storage="MB">10</Size>
		<NoOfFile>5</NoOfFile>
	</Logging>
</configuration>

--MIME_boundary--